{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":43,"n_cols":9,"rows_kept":43,"merged":[[0,0,0,8],[3,0,11,0],[3,1,8,1],[3,7,11,7],[3,8,11,8],[12,0,17,0],[12,1,14,1],[12,2,14,2],[12,7,17,7],[12,8,17,8],[18,0,22,0],[18,1,20,1],[18,7,22,7],[18,8,22,8],[23,0,27,0],[23,1,25,1],[23,2,25,2],[23,7,27,7],[23,8,27,8],[28,0,31,0],[28,1,29,1],[28,7,31,7],[28,8,31,8],[32,0,35,0],[32,7,35,7],[32,8,35,8],[36,0,37,0],[36,7,37,7],[36,8,37,8],[38,0,42,0],[38,7,42,7],[38,8,42,8]],"flags":["formulas_cached_only"]}
["建龙北满特钢危险废物管理责任分工情况表"]
["单位：建龙北满特殊钢有限责任公司"]
["产废单位","涉及危废名称","危废类别","危废代码","危废特性","产生环节","危废去向","管理责任人","联系方式"]
["轧钢厂","废矿物油与含矿物油废物","HW08","900-218-08","T","液压设备维护、更换和拆解过程中产生的废液压油","过滤后回用，无法回用的用于链条润滑","张洪娟",18904079083]
[null,null,"HW08","900-217-08","T","轧机设备润滑产生的废润滑油","用于转移链条润滑"]
[null,null,"HW08","900-213-08","T、I","滤油后产生的过滤残渣","转移至采购危废库房暂存、待统一转移至有资质第三方处置"]
[null,null,"HW08","900-249-08","T","设备辊道润滑产生的废锂基脂","确认无利用价值可收集暂存，统一转移至有资质第三方进行无害化处置"]
[null,null,"HW08","900-249-08","T","使用矿物油剩余空油桶","炼钢综合利用"]
[null,null,"HW08","900-249-08","T","预精轧、精轧过程中产生的油膜轴承油","用于油气润滑"]
[null,"含油废布","HW49","900-041-49","T、I","作业过程中沾染废矿物油的含油抹布、劳保用品。","未统一收集的、随生活垃圾一同处置，统一收集的需报告入库并转移有资质第三方处置"]
[null,"废油桶","HW49","900-041-49","T","盛装过废矿物油的油桶","重复使用、无法使用后统一收集报告，转移至有资质第三方进行无害化处置"]
[null,"废铅蓄电池","HW31","900-052-31","T、C","天车或备用电源更换铅蓄电池产生","转移至采购危废库房暂存、待统一转移至有资质第三方处置"]
["特冶锻造厂","废矿物油与含矿物油废物","HW08","900-218-08","T、I","液压设备维护、更换和拆解过程中产生的废液压油","过滤后回用，无法回用的用作线上润滑或淬火油池利用","李刚",15946230459]
[{"$nulls":3},"900-213-08","T、I","滤油后产生的过滤残渣","转移至采购危废库房暂存、待统一转移至有资质第三方处置"]
[{"$nulls":3},"900-249-08","T","使用矿物油剩余空油桶","炼钢综合利用"]
[null,"含油废布","HW49","900-041-49","T、I","作业过程中沾染废矿物油的含油抹布、劳保用品。","未统一收集的、随生活垃圾一同处置，统一收集的需报告入库并转移有资质第三方处置"]
[null,"废油桶","HW49","900-041-49","T","盛装过废矿物油的油桶","重复使用、无法使用后统一收集报告，转移至有资质第三方进行无害化处置"]
[null,"沾染乳化液钢屑","HW09","900-006-09","T","使用切削油和切削液进行机械加工过程中产生的含乳化液钢屑。","炼钢综合利用"]
["炼铁厂","废矿物油与含矿物油废物","HW08","900-218-08","T","液压设备维护产生的废液压油","过滤后回用，无法回用的用作辊道润滑","徐晓宇",13604614763]
[null,null,"HW08","900-217-08","T、I","喷煤润滑站、高炉主卷扬等大修时更换的废润滑油","过滤后回用或用于稀油润滑，确认无利用价值的暂存转至有资质第三方处置。"]
[null,null,"HW08","900-249-08","T","使用矿物油剩余空油桶","炼钢综合利用"]
[null,"废油桶","HW49","900-041-49","T","盛装过废矿物油的油桶","重复使用、无法使用后统一收集报告，转移至有资质第三方进行无害化处置"]
[null,"含油废布","HW49","900-041-49","T、I","作业过程中沾染废矿物油的含油抹布、劳保用品。","未统一收集的、随生活垃圾一同处置，统一收集的需报告入库并转移有资质第三方处置"]
["能源中心","废矿物油与含矿物油废物","HW08","900-217-08","T、I","机械设备润滑过程中产生的废润滑油","过滤后回用，无法再次使用的贮存转至有资质第三方处置。","张博",13796850015]
[{"$nulls":3},"900-220-08","T","变压器维护、更换和拆解过程中产生的废变压器油","过滤后回用"]
[{"$nulls":3},"900-249-08","T","使用矿物油剩余空油桶","炼钢综合利用"]
[null,"废铅蓄电池","HW31","900-052-31","T、C","各总降UPS电源更换产生","转至采购部危废库房贮存"]
[null,"监测废液","HW49","900-047-49","T、C、R","废水自动在线监测设备化验分析产生的废液。","转至采购部危废库房贮存"]
["一炼钢厂","废矿物油与含矿物油废物","HW08","900-218-08","T","液压设备维护产生的废液压油","过滤后回用，无法回用液压系统的用作线上润滑或淬火油池利用","盖鑫",13845214007]
[null,null,"HW08","900-249-08","T","使用矿物油剩余空油桶","炼钢综合利用"]
[null,"废铅蓄电池","HW31","900-052-31","T、C","天车铅蓄电池更换产生","转至采购部危废库房贮存"]
[null,"含油废布","HW49","900-041-49","T、I","作业过程中沾染废矿物油的含油抹布、劳保用品。","未统一收集的、随生活垃圾一同处置，统一收集的需报告入库并转移有资质第三方处置"]
["质量部","废药品瓶","HW49","900-041-49","T","实验剩余空药品瓶","转至采购部危废库房贮存","褚庆雨",13796344433]
[null,"有机废液","HW49","900-047-49","T","实验过程产生的有机废液","转至采购部危废库房贮存"]
[null,"沾染乳化液钢屑","HW09","900-006-09","T","使用切削油和切削液进行机械加工过程中产生的含乳化液钢屑。","返回炼钢综合利用"]
[null,"含油废布","HW49","900-041-49","T、I","作业过程中沾染废矿物油的含油抹布、劳保用品。","未统一收集的、随生活垃圾一同处置，统一收集的需报告入库并转移有资质第三方处置"]
["工程装备部","含油废布","HW49","900-041-49","T、I","作业过程中沾染废矿物油的含油抹布、劳保用品。","未统一收集的、随生活垃圾一同处置，统一收集的需报告入库并转移有资质第三方处置","吴昊",13763567100]
[null,"沾染乳化液钢屑","HW09","900-006-09","T","机床加工过程产生","返回炼钢综合利用"]
["采购部","废铅蓄电池","HW49","900-052-31","T、C","危废库房贮存","贮存、定期转至有资质第三方处置","高玲玲",13796249742]
[null,"化验废液","HW49","900-047-49","T、R","危废库房贮存","贮存、定期转至有资质第三方处置"]
[null,"滤油残渣","HW08","900-213-08","T、I","危废库房贮存","贮存、定期转至有资质第三方处置"]
[null,"有机废液","HW49","900-047-49","T","危废库房贮存","贮存、定期转至有资质第三方处置"]
[null,"废药品瓶","HW49","900-041-49","T","危废库房贮存","贮存、定期转至有资质第三方处置"]